number of wire

2 4 6 8 10 12 mean value of the res (cm)

-0.15

-0.1

-0.05

-0

0.05

0.1

0.15

Cam 2 int: GARFIELD with angle correction (red) garfield (black)

number of wire

2 4 6 8 10 12 mean value of the res (cm)

-0.15

-0.1

-0.05

-0

0.05

0.1

0.15

Cam 6 int: GARFIELD with angle correction (red) garfield (black)

number of wire

2 4 6 8 10 12 mean value of the res (cm)

-0.15

-0.1

-0.05

-0

0.05

0.1

0.15

Cam 3 est: GARFIELD with angle correction (red) garfield (black)

number of wire

2 4 6 8 10 12 mean value of the res (cm)

-0.15

-0.1

-0.05

-0

0.05

0.1

0.15

Cam 7 est: GARFIELD with angle correction (red) garfield (black)